{"text_format":"1","workbook":"xlsx","n_sheets":16,"sheets":["Vars","Schließplan","Listen","Bravus.2500 MX","Bravus.3500 MX","Bravus.2000","Bravus.3000","Bravus.4000","Vitess.1000","Vitess.2000","Vitess.4000","Wavy Line Pro","Wilka Carat S1","Wilka Carat S3","CES UDM","CES RHM"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Vars","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"Schließplan","index":1,"n_rows":15,"n_cols":13,"rows_kept":15,"cut":false,"hidden":false,"merged":[[14,10,14,11],[10,10,10,11],[11,0,11,11],[11,12,13,12],[12,0,13,0],[12,1,13,1],[12,3,13,3],[12,10,13,11],[12,4,12,5],[12,6,13,6],[12,7,13,7],[12,8,13,9],[8,5,8,6],[0,9,8,9],[9,9,10,9],[1,12,6,12],[1,10,6,11],[6,5,6,6],[7,12,9,12],[7,10,9,11],[1,1,1,5],[5,1,5,4],[4,1,4,4],[7,5,7,6],[3,1,3,4]]}
[null,"Der EXPERTE für Sicherheit - Schließanlagen und Schließzylinder",null,null,null,null,null,null,null,"S  c  h  l  ü  s  s  e  l",null,null,1]
[null,"Service- & Bestell-Hotline: +49 (0)821 899 493-0 (Mo.- Fr. 9:30 - 17:30 Uhr)\nEmail: vertrieb@expert-security.de",null,null,null,null,null,"  ",null,null,"Zusatzbezeichnung"]
[null,null,null,null,null,null,"Angebot-Nr.:"]
["Firma:",null,null,null,null,null,"Kommission:"]
["Name / AP:",null,null,null,null,null,"Anlage-Nr.:"]
["E-Mail:",null,null,null,null,null,"Objekt:"]
["Bestell-Nr.:",null,null,"Kundennummer:",null,"Sind in Zukunft weitere Zylinder geplant?"]
["System:",null,null,null,null,"Sind in Zukunft weitere Schlüssel geplant?",null,null,null,null,"Bez.",null,"Schlüssel 1"]
[]
["Bemerkungen:"]
[null,null,null,null,null,null,null,null,null,null,"Anzahl"]
["Z  y  l  i  n  d  e  r "]
["Position","Tür- oder Raumbezeichnung",null,"Zylinder-Typ","Zylinderlänge in mm",null,"Not- und Gefahrenfunktion i","Bohrschutz i","Modell",null,"Anzahl"]
[null,null,"Zylinder Artikel-Nr.",null,"außen","innen i"]
[1,"Tür 1"]

{"sheet":"Listen","index":2,"n_rows":16,"n_cols":6,"rows_kept":16,"cut":false,"hidden":true,"merged":[]}
[]
[]
[null,"Typ",null,"Weitere Zylinder",null,"Weitere Schlüssel"]
[null,"Bravus.2000",null,"nein",null,"nein"]
[null,"Bravus.3000",null,"ja",null,"ja"]
[null,"Bravus.4000",null,"1-5 Zylinder",null,"1-5 Schlüssel"]
[null,"Bravus.2500 MX",null,"5-10 Zylinder",null,"5-10 Schlüssel"]
[null,"Bravus.3500 MX",null,"10-15 Zylinder",null,"10-15 Schlüssel"]
[null,"Wavy Line Pro",null,"15-20 Zylinder",null,"15-20 Schlüssel"]
[null,"Vitess.1000"]
[null,"Vitess.2000"]
[null,"Vitess.4000"]
[null,"CES UDM"]
[null,"CES RHM"]
[null,"Wilka Carat S1"]
[null,"Wilka Carat S3"]

{"sheet":"Bravus.2500 MX","index":3,"n_rows":42,"n_cols":13,"rows_kept":42,"cut":false,"hidden":true,"merged":[]}
["Typ",null,"Doppelzylinder",null,"Knaufzylinder",null,"Halbzylinder",null,"Vorhangschloss",null,"Außenzylinder",null,"Hebelzylinder"]
["Doppelzylinder"]
["Knaufzylinder",null,"außen",null,"außen",null,"außen",null,"Modell",null,null,null,"Modell"]
["Halbzylinder",null,30,null,30,null,30,null,"Bügelhöhe 28 mm",null,null,null,"Ø 24 mm"]
["Vorhangschloss",null,35,null,35,null,35,null,"Schließeinsatz 86er Serie",null,null,null,"Ø 27 mm"]
["Außenzylinder",null,40,null,40,null,40]
["Hebelzylinder",null,45,null,45,null,45]
[null,null,50,null,50,null,50]
[null,null,55,null,55,null,55]
[null,null,60,null,60,null,60]
[null,null,65,null,65,null,65]
[null,null,70,null,70,null,70]
[]
[]
[]
[]
[]
[]
[]
[null,null,"innen",null,"innen",null,"innen"]
[null,null,30,null,30,null,10]
[null,null,35,null,35]
[null,null,40,null,40]
[null,null,45,null,45]
[null,null,50,null,50]
[null,null,55,null,55]
[null,null,60,null,60]
[null,null,65,null,65]
[null,null,70,null,70]
[]
[]
[]
[]
[null,null,"NGF",null,"NGF",null,"NGF"]
[null,null,"ohne Not- und Gefahrenfunktion",null,"nur für Doppelzylinder",null,"nur für Doppelzylinder"]
[null,null,"mit Not- und Gefahrenfunktion"]
[null,null,"mit Freilauffunktion"]
[]
[]
[]
[null,null,"Bohrschutz",null,"Bohrschutz",null,"Bohrschutz"]
[null,null,"Serienmäßig höchste SKG*** Zertifizierung",null,"Serienmäßig höchste SKG*** Zertifizierung",null,"Serienmäßig höchste SKG*** Zertifizierung"]

{"sheet":"Bravus.3500 MX","index":4,"n_rows":42,"n_cols":13,"rows_kept":42,"cut":false,"hidden":true,"merged":[]}
["Typ",null,"Doppelzylinder",null,"Knaufzylinder",null,"Halbzylinder",null,"Vorhangschloss",null,"Außenzylinder",null,"Hebelzylinder"]
["Doppelzylinder"]
["Knaufzylinder",null,"außen",null,"außen",null,"außen",null,"Modell",null,null,null,"Modell"]
["Halbzylinder",null,30,null,30,null,30,null,"Bügelhöhe 28 mm",null,null,null,"Ø 24 mm"]
["Vorhangschloss",null,35,null,35,null,35,null,"Schließeinsatz 86er Serie",null,null,null,"Ø 27 mm"]
["Außenzylinder",null,40,null,40,null,40]
["Hebelzylinder",null,45,null,45,null,45]
[null,null,50,null,50,null,50]
[null,null,55,null,55,null,55]
[null,null,60,null,60,null,60]
[null,null,65,null,65,null,65]
[null,null,70,null,70,null,70]
[]
[]
[]
[]
[]
[]
[]
[null,null,"innen",null,"innen",null,"innen"]
[null,null,30,null,30,null,10]
[null,null,35,null,35]
[null,null,40,null,40]
[null,null,45,null,45]
[null,null,50,null,50]
[null,null,55,null,55]
[null,null,60,null,60]
[null,null,65,null,65]
[null,null,70,null,70]
[]
[]
[]
[]
[null,null,"NGF",null,"NGF",null,"NGF"]
[null,null,"ohne Not- und Gefahrenfunktion",null,"nur für Doppelzylinder",null,"nur für Doppelzylinder"]
[null,null,"mit Not- und Gefahrenfunktion"]
[null,null,"mit Freilauffunktion"]
[]
[]
[]
[null,null,"Bohrschutz",null,"Bohrschutz",null,"Bohrschutz"]
[null,null,"Serienmäßig höchste SKG*** Zertifizierung",null,"Serienmäßig höchste SKG*** Zertifizierung",null,"Serienmäßig höchste SKG*** Zertifizierung"]

{"sheet":"Bravus.2000","index":5,"n_rows":43,"n_cols":13,"rows_kept":43,"cut":false,"hidden":true,"merged":[]}
["Typ",null,"Doppelzylinder",null,"Knaufzylinder",null,"Halbzylinder",null,"Vorhangschloss",null,"Außenzylinder",null,"Hebelzylinder"]
["Doppelzylinder"]
["Knaufzylinder",null,"außen",null,"außen",null,"außen",null,"Modell",null,null,null,"Modell"]
["Halbzylinder",null,30,null,30,null,30,null,"Bügelhöhe 28 mm",null,null,null,"Ø 24 mm"]
["Vorhangschloss",null,35,null,35,null,35,null,"86TI/45",null,null,null,"Ø 27 mm"]
["Außenzylinder",null,40,null,40,null,40]
["Hebelzylinder",null,45,null,45,null,45]
[null,null,50,null,50,null,50]
[null,null,55,null,55,null,55]
[null,null,60,null,60,null,60]
[null,null,65,null,65,null,65]
[null,null,70,null,70,null,70]
[]
[]
[]
[]
[]
[]
[]
[null,null,"innen",null,"innen",null,"innen"]
[null,null,30,null,30,null,10]
[null,null,35,null,35]
[null,null,40,null,40]
[null,null,45,null,45]
[null,null,50,null,50]
[null,null,55,null,55]
[null,null,60,null,60]
[null,null,65,null,65]
[null,null,70,null,70]
[]
[]
[]
[]
[null,null,"NGF",null,"NGF",null,"NGF"]
[null,null,"ohne Not- und Gefahrenfunktion",null,"nur für Doppelzylinder",null,"nur für Doppelzylinder"]
[null,null,"mit Not- und Gefahrenfunktion"]
[null,null,"mit Freilauffunktion"]
[]
[]
[]
[null,null,"Bohrschutz",null,"Bohrschutz",null,"Bohrschutz"]
[null,null,"erhöhter Bohrschutz (BS01)",null,"erhöhter Bohrschutz (BS01)",null,"erhöhter Bohrschutz (BS01)"]
[null,null,"hochfester Bohrschutz (BS04)",null,"hochfester Bohrschutz (BS04)",null,"hochfester Bohrschutz (BS04)"]

{"sheet":"Bravus.3000","index":6,"n_rows":43,"n_cols":13,"rows_kept":43,"cut":false,"hidden":true,"merged":[]}
["Typ",null,"Doppelzylinder",null,"Knaufzylinder",null,"Halbzylinder",null,"Vorhangschloss",null,"Außenzylinder",null,"Hebelzylinder"]
["Doppelzylinder"]
["Knaufzylinder",null,"außen",null,"außen",null,"außen",null,"Modell",null,null,null,"Modell"]
["Halbzylinder",null,30,null,30,null,30,null,"Bügelhöhe 28 mm",null,null,null,"Ø 24 mm"]
["Vorhangschloss",null,35,null,35,null,35,null,"86TI/45",null,null,null,"Ø 27 mm"]
["Außenzylinder",null,40,null,40,null,40]
["Hebelzylinder",null,45,null,45,null,45]
[null,null,50,null,50,null,50]
[null,null,55,null,55,null,55]
[null,null,60,null,60,null,60]
[null,null,65,null,65,null,65]
[null,null,70,null,70,null,70]
[]
[]
[]
[]
[]
[]
[]
[null,null,"innen",null,"innen",null,"innen"]
[null,null,30,null,30,null,10]
[null,null,35,null,35]
[null,null,40,null,40]
[null,null,45,null,45]
[null,null,50,null,50]
[null,null,55,null,55]
[null,null,60,null,60]
[null,null,65,null,65]
[null,null,70,null,70]
[]
[]
[]
[]
[null,null,"NGF",null,"NGF",null,"NGF"]
[null,null,"ohne Not- und Gefahrenfunktion",null,"nur für Doppelzylinder",null,"nur für Doppelzylinder"]
[null,null,"mit Not- und Gefahrenfunktion"]
[null,null,"mit Freilauffunktion"]
[]
[]
[]
[null,null,"Bohrschutz",null,"Bohrschutz",null,"Bohrschutz"]
[null,null,"erhöhter Bohrschutz (BS01)",null,"erhöhter Bohrschutz (BS01)",null,"erhöhter Bohrschutz (BS01)"]
[null,null,"hochfester Bohrschutz (BS04)",null,"hochfester Bohrschutz (BS04)",null,"hochfester Bohrschutz (BS04)"]

{"sheet":"Bravus.4000","index":7,"n_rows":43,"n_cols":13,"rows_kept":43,"cut":false,"hidden":true,"merged":[]}
["Typ",null,"Doppelzylinder",null,"Knaufzylinder",null,"Halbzylinder",null,"Vorhangschloss",null,"Außenzylinder",null,"Hebelzylinder"]
["Doppelzylinder"]
["Knaufzylinder",null,"außen",null,"außen",null,"außen",null,"Modell",null,null,null,"Modell"]
["Halbzylinder",null,30,null,30,null,30,null,"Bügelhöhe 28 mm",null,null,null,"Ø 24 mm"]
["Vorhangschloss",null,35,null,35,null,35,null,"86TI/45",null,null,null,"Ø 27 mm"]
["Außenzylinder",null,40,null,40,null,40]
["Hebelzylinder",null,45,null,45,null,45]
[null,null,50,null,50,null,50]
[null,null,55,null,55,null,55]
[null,null,60,null,60,null,60]
[null,null,65,null,65,null,65]
[null,null,70,null,70,null,70]
[]
[]
[]
[]
[]
[]
[]
[null,null,"innen",null,"innen",null,"innen"]
[null,null,30,null,30,null,10]
[null,null,35,null,35]
[null,null,40,null,40]
[null,null,45,null,45]
[null,null,50,null,50]
[null,null,55,null,55]
[null,null,60,null,60]
[null,null,65,null,65]
[null,null,70,null,70]
[]
[]
[]
[]
[null,null,"NGF",null,"NGF",null,"NGF"]
[null,null,"ohne Not- und Gefahrenfunktion",null,"nur für Doppelzylinder",null,"nur für Doppelzylinder"]
[null,null,"mit Not- und Gefahrenfunktion"]
[null,null,"mit Freilauffunktion"]
[]
[]
[]
[null,null,"Bohrschutz",null,"Bohrschutz",null,"Bohrschutz"]
[null,null,"erhöhter Bohrschutz (BS01)",null,"erhöhter Bohrschutz (BS01)",null,"erhöhter Bohrschutz (BS01)"]
[null,null,"hochfester Bohrschutz (BS04)",null,"hochfester Bohrschutz (BS04)",null,"hochfester Bohrschutz (BS04)"]

{"sheet":"Vitess.1000","index":8,"n_rows":43,"n_cols":13,"rows_kept":43,"cut":false,"hidden":true,"merged":[]}
["Typ",null,"Doppelzylinder",null,"Knaufzylinder",null,"Halbzylinder",null,"Vorhangschloss",null,"Außenzylinder",null,"Hebelzylinder"]
["Doppelzylinder"]
["Knaufzylinder",null,"außen",null,"außen",null,"außen",null,"Modell",null,null,null,"Modell"]
["Halbzylinder",null,30,null,30,null,30,null,"Bügelhöhe 28 mm",null,null,null,"Ø 24 mm"]
["Vorhangschloss",null,35,null,35,null,35,null,"86TI/45",null,null,null,"Ø 27 mm"]
["Außenzylinder",null,40,null,40,null,40]
["Hebelzylinder",null,45,null,45,null,45]
[null,null,50,null,50,null,50]
[null,null,55,null,55,null,55]
[null,null,60,null,60,null,60]
[null,null,65,null,65,null,65]
[null,null,70,null,70,null,70]
[]
[]
[]
[]
[]
[]
[]
[null,null,"innen",null,"innen",null,"innen"]
[null,null,30,null,30,null,10]
[null,null,35,null,35]
[null,null,40,null,40]
[null,null,45,null,45]
[null,null,50,null,50]
[null,null,55,null,55]
[null,null,60,null,60]
[null,null,65,null,65]
[null,null,70,null,70]
[]
[]
[]
[]
[null,null,"NGF",null,"NGF",null,"NGF"]
[null,null,"ohne Not- und Gefahrenfunktion",null,"nur für Doppelzylinder",null,"nur für Doppelzylinder"]
[null,null,"mit Not- und Gefahrenfunktion"]
[null,null,"mit Freilauffunktion"]
[]
[]
[]
[null,null,"Bohrschutz",null,"Bohrschutz",null,"Bohrschutz"]
[null,null,"erhöhter Bohrschutz (BS01)",null,"erhöhter Bohrschutz (BS01)",null,"erhöhter Bohrschutz (BS01)"]
[null,null,"hochfester Bohrschutz (BS04)",null,"hochfester Bohrschutz (BS04)",null,"hochfester Bohrschutz (BS04)"]

{"sheet":"Vitess.2000","index":9,"n_rows":43,"n_cols":13,"rows_kept":43,"cut":false,"hidden":true,"merged":[]}
["Typ",null,"Doppelzylinder",null,"Knaufzylinder",null,"Halbzylinder",null,"Vorhangschloss",null,"Außenzylinder",null,"Hebelzylinder"]
["Doppelzylinder"]
["Knaufzylinder",null,"außen",null,"außen",null,"außen",null,"Modell",null,null,null,"Modell"]
["Halbzylinder",null,30,null,30,null,30,null,"Bügelhöhe 28 mm",null,null,null,"Ø 24 mm"]
["Vorhangschloss",null,35,null,35,null,35,null,"86TI/45",null,null,null,"Ø 27 mm"]
["Außenzylinder",null,40,null,40,null,40]
["Hebelzylinder",null,45,null,45,null,45]
[null,null,50,null,50,null,50]
[null,null,55,null,55,null,55]
[null,null,60,null,60,null,60]
[null,null,65,null,65,null,65]
[null,null,70,null,70,null,70]
[]
[]
[]
[]
[]
[]
[]
[null,null,"innen",null,"innen",null,"innen"]
[null,null,30,null,30,null,10]
[null,null,35,null,35]
[null,null,40,null,40]
[null,null,45,null,45]
[null,null,50,null,50]
[null,null,55,null,55]
[null,null,60,null,60]
[null,null,65,null,65]
[null,null,70,null,70]
[]
[]
[]
[]
[null,null,"NGF",null,"NGF",null,"NGF"]
[null,null,"ohne Not- und Gefahrenfunktion",null,"nur für Doppelzylinder",null,"nur für Doppelzylinder"]
[null,null,"mit Not- und Gefahrenfunktion"]
[null,null,"mit Freilauffunktion"]
[]
[]
[]
[null,null,"Bohrschutz",null,"Bohrschutz",null,"Bohrschutz"]
[null,null,"erhöhter Bohrschutz (BS01)",null,"erhöhter Bohrschutz (BS01)",null,"erhöhter Bohrschutz (BS01)"]
[null,null,"hochfester Bohrschutz (BS04)",null,"hochfester Bohrschutz (BS04)",null,"hochfester Bohrschutz (BS04)"]

{"sheet":"Vitess.4000","index":10,"n_rows":43,"n_cols":13,"rows_kept":43,"cut":false,"hidden":true,"merged":[]}
["Typ",null,"Doppelzylinder",null,"Knaufzylinder",null,"Halbzylinder",null,"Vorhangschloss",null,"Außenzylinder",null,"Hebelzylinder"]
["Doppelzylinder"]
["Knaufzylinder",null,"außen",null,"außen",null,"außen",null,"Modell",null,null,null,"Modell"]
["Halbzylinder",null,30,null,30,null,30,null,"Bügelhöhe 28 mm",null,null,null,"Ø 24 mm"]
["Vorhangschloss",null,35,null,35,null,35,null,"86TI/45",null,null,null,"Ø 27 mm"]
["Außenzylinder",null,40,null,40,null,40]
["Hebelzylinder",null,45,null,45,null,45]
[null,null,50,null,50,null,50]
[null,null,55,null,55,null,55]
[null,null,60,null,60,null,60]
[null,null,65,null,65,null,65]
[null,null,70,null,70,null,70]
[]
[]
[]
[]
[]
[]
[]
[null,null,"innen",null,"innen",null,"innen"]
[null,null,30,null,30,null,10]
[null,null,35,null,35]
[null,null,40,null,40]
[null,null,45,null,45]
[null,null,50,null,50]
[null,null,55,null,55]
[null,null,60,null,60]
[null,null,65,null,65]
[null,null,70,null,70]
[]
[]
[]
[]
[null,null,"NGF",null,"NGF",null,"NGF"]
[null,null,"ohne Not- und Gefahrenfunktion",null,"nur für Doppelzylinder",null,"nur für Doppelzylinder"]
[null,null,"mit Not- und Gefahrenfunktion"]
[null,null,"mit Freilauffunktion"]
[]
[]
[]
[null,null,"Bohrschutz",null,"Bohrschutz",null,"Bohrschutz"]
[null,null,"erhöhter Bohrschutz (BS01)",null,"erhöhter Bohrschutz (BS01)",null,"erhöhter Bohrschutz (BS01)"]
[null,null,"hochfester Bohrschutz (BS04)",null,"hochfester Bohrschutz (BS04)",null,"hochfester Bohrschutz (BS04)"]

{"sheet":"Wavy Line Pro","index":11,"n_rows":43,"n_cols":13,"rows_kept":43,"cut":false,"hidden":true,"merged":[]}
["Typ",null,"Doppelzylinder",null,"Knaufzylinder",null,"Halbzylinder",null,"Vorhangschloss",null,"Außenzylinder",null,"Hebelzylinder"]
["Doppelzylinder"]
["Knaufzylinder",null,"außen",null,"außen",null,"außen",null,"Modell",null,null,null,"Modell"]
["Halbzylinder",null,30,null,30,null,30,null,"Schließeinastz für VHS83",null,null,null,"Ø 24 mm"]
["Vorhangschloss",null,35,null,35,null,35]
["Außenzylinder",null,40,null,40,null,40]
["Hebelzylinder",null,45,null,45,null,45]
[null,null,50,null,50,null,50]
[null,null,55,null,55,null,55]
[null,null,60,null,60,null,60]
[null,null,65,null,65,null,65]
[null,null,70,null,70,null,70]
[]
[]
[]
[]
[]
[]
[]
[null,null,"innen",null,"innen",null,"innen"]
[null,null,30,null,30,null,10]
[null,null,35,null,35]
[null,null,40,null,40]
[null,null,45,null,45]
[null,null,50,null,50]
[null,null,55,null,55]
[null,null,60,null,60]
[null,null,65,null,65]
[null,null,70,null,70]
[]
[]
[]
[]
[null,null,"NGF",null,"NGF",null,"NGF"]
[null,null,"ohne Not- und Gefahrenfunktion",null,"nur für Doppelzylinder",null,"nur für Doppelzylinder"]
[null,null,"mit Not- und Gefahrenfunktion"]
[null,null,"mit Freilauffunktion"]
[]
[]
[]
[null,null,"Bohrschutz",null,"Bohrschutz",null,"Bohrschutz"]
[null,null,"erhöhter Bohrschutz (BS01)",null,"erhöhter Bohrschutz (BS01)",null,"erhöhter Bohrschutz (BS01)"]
[null,null,"hochfester Bohrschutz (BS04)",null,"hochfester Bohrschutz (BS04)",null,"hochfester Bohrschutz (BS04)"]

{"sheet":"Wilka Carat S1","index":12,"n_rows":43,"n_cols":13,"rows_kept":43,"cut":false,"hidden":true,"merged":[]}
["Typ",null,"Doppelzylinder",null,"Knaufzylinder",null,"Halbzylinder",null,"Vorhangschloss",null,"Außenzylinder",null,"Hebelzylinder"]
["Doppelzylinder"]
["Knaufzylinder",null,"außen",null,"außen",null,"außen",null,"Modell",null,null,null,"Modell"]
["Halbzylinder",null,30,null,30,null,30,null,"Bügelhöhe 30mm",null,null,null,"90°"]
["Vorhangschloss",null,35,null,35,null,35]
["Außenzylinder",null,40,null,40,null,40]
["Hebelzylinder",null,45,null,45,null,45]
[null,null,50,null,50,null,50]
[null,null,55,null,55,null,55]
[null,null,60,null,60,null,60]
[null,null,65,null,65,null,65]
[null,null,70,null,70,null,70]
[]
[]
[]
[]
[]
[]
[]
[null,null,"innen",null,"innen",null,"innen"]
[null,null,30,null,30,null,10]
[null,null,35,null,35]
[null,null,40,null,40]
[null,null,45,null,45]
[null,null,50,null,50]
[null,null,55,null,55]
[null,null,60,null,60]
[null,null,65,null,65]
[null,null,70,null,70]
[]
[]
[]
[]
[null,null,"NGF",null,"NGF",null,"NGF"]
[null,null,"ohne Not- und Gefahrenfunktion",null,"nur für Doppelzylinder",null,"nur für Doppelzylinder"]
[null,null,"mit Not- und Gefahrenfunktion"]
[null,null,"mit Freilauffunktion"]
[]
[]
[]
[null,null,"Bohrschutz",null,"Bohrschutz",null,"Bohrschutz"]
[null,null,"Anbohrhemmung I",null,"Anbohrhemmung I",null,"Anbohrhemmung I"]
[null,null,"Anbohrhemmung III",null,"Anbohrhemmung III",null,"Anbohrhemmung III"]

{"sheet":"Wilka Carat S3","index":13,"n_rows":43,"n_cols":13,"rows_kept":43,"cut":false,"hidden":true,"merged":[]}
["Typ",null,"Doppelzylinder",null,"Knaufzylinder",null,"Halbzylinder",null,"Vorhangschloss",null,"Außenzylinder",null,"Hebelzylinder"]
["Doppelzylinder"]
["Knaufzylinder",null,"außen",null,"außen",null,"außen",null,"Modell",null,null,null,"Modell"]
["Halbzylinder",null,30,null,30,null,30,null,"Bügelhöhe 30mm",null,null,null,"90°"]
["Vorhangschloss",null,35,null,35,null,35]
["Außenzylinder",null,40,null,40,null,40]
["Hebelzylinder",null,45,null,45,null,45]
[null,null,50,null,50,null,50]
[null,null,55,null,55,null,55]
[null,null,60,null,60,null,60]
[null,null,65,null,65,null,65]
[null,null,70,null,70,null,70]
[]
[]
[]
[]
[]
[]
[]
[null,null,"innen",null,"innen",null,"innen"]
[null,null,30,null,30,null,10]
[null,null,35,null,35]
[null,null,40,null,40]
[null,null,45,null,45]
[null,null,50,null,50]
[null,null,55,null,55]
[null,null,60,null,60]
[null,null,65,null,65]
[null,null,70,null,70]
[]
[]
[]
[]
[null,null,"NGF",null,"NGF",null,"NGF"]
[null,null,"ohne Not- und Gefahrenfunktion",null,"nur für Doppelzylinder",null,"nur für Doppelzylinder"]
[null,null,"mit Not- und Gefahrenfunktion"]
[null,null,"mit Freilauffunktion"]
[]
[]
[]
[null,null,"Bohrschutz",null,"Bohrschutz",null,"Bohrschutz"]
[null,null,"Anbohrhemmung IX",null,"Anbohrhemmung IX",null,"Anbohrhemmung IX"]
[null,null,"Anbohrhemmung X",null,"Anbohrhemmung X",null,"Anbohrhemmung X"]

{"sheet":"CES UDM","index":14,"n_rows":45,"n_cols":13,"rows_kept":45,"cut":false,"hidden":true,"merged":[]}
["Typ",null,"Doppelzylinder",null,"Knaufzylinder",null,"Halbzylinder",null,"Vorhangschloss",null,"Außenzylinder",null,"Hebelzylinder"]
["Doppelzylinder"]
["Knaufzylinder",null,"außen",null,"außen",null,"außen",null,"Modell",null,null,null,"Modell"]
["Halbzylinder",null,30,null,30,null,30,null,"215N/58 - Bügelhöhe 35",null,null,null,"5558/30"]
["Vorhangschloss",null,35,null,35,null,35,null,"215N/58 - Bügelhöhe 45"]
["Außenzylinder",null,40,null,40,null,40,null,"215N/58 - Bügelhöhe 55"]
["Hebelzylinder",null,45,null,45,null,45,null,"215N/58 - Bügelhöhe 65"]
[null,null,50,null,50,null,50,null,"215N/58 - Bügelhöhe 75"]
[null,null,55,null,55,null,55,null,"215N/58 - Bügelhöhe 105"]
[null,null,60,null,60,null,60,null,"215N/58 - Bügelhöhe 205"]
[null,null,65,null,65,null,65]
[null,null,70,null,70,null,70]
[]
[]
[]
[]
[]
[]
[]
[null,null,"innen",null,"innen",null,"innen"]
[null,null,30,null,30,null,10]
[null,null,35,null,35]
[null,null,40,null,40]
[null,null,45,null,45]
[null,null,50,null,50]
[null,null,55,null,55]
[null,null,60,null,60]
[null,null,65,null,65]
[null,null,70,null,70]
[]
[]
[]
[]
[null,null,"NGF",null,"NGF",null,"NGF"]
[null,null,"ohne Not- und Gefahrenfunktion",null,"nur für Doppelzylinder",null,"nur für Doppelzylinder"]
[null,null,"mit Not- und Gefahrenfunktion"]
[null,null,"mit Freilauffunktion"]
[]
[]
[]
[null,null,"Bohrschutz",null,"Bohrschutz",null,"Bohrschutz"]
[null,null,"Bohrschutz Klasse 3 (BS3)",null,"Bohrschutz Klasse 3 (BS3)",null,"Bohrschutz Klasse 3 (BS3)"]
[null,null,"Bohrschutz Klasse 4 (BS4)",null,"Bohrschutz Klasse 4 (BS4)",null,"Bohrschutz Klasse 4 (BS4)"]
[null,null,"Bohr- und Ziehschutz (BZ1)",null,"Bohr- und Ziehschutz (BZ1)",null,"Bohr- und Ziehschutz (BZ1)"]
[null,null,"Bohr- und Ziehschutz (BZ2)",null,"Bohr- und Ziehschutz (BZ2)",null,"Bohr- und Ziehschutz (BZ2)"]

{"sheet":"CES RHM","index":15,"n_rows":45,"n_cols":13,"rows_kept":45,"cut":false,"hidden":true,"merged":[]}
["Typ",null,"Doppelzylinder",null,"Knaufzylinder",null,"Halbzylinder",null,"Vorhangschloss",null,"Außenzylinder",null,"Hebelzylinder"]
["Doppelzylinder"]
["Knaufzylinder",null,"außen",null,"außen",null,"außen",null,"Modell",null,null,null,"Modell"]
["Halbzylinder",null,30,null,30,null,30,null,"215N/58 - Bügelhöhe 35",null,null,null,"5558/30"]
["Vorhangschloss",null,35,null,35,null,35,null,"215N/58 - Bügelhöhe 45"]
["Außenzylinder",null,40,null,40,null,40,null,"215N/58 - Bügelhöhe 55"]
["Hebelzylinder",null,45,null,45,null,45,null,"215N/58 - Bügelhöhe 65"]
[null,null,50,null,50,null,50,null,"215N/58 - Bügelhöhe 75"]
[null,null,55,null,55,null,55,null,"215N/58 - Bügelhöhe 105"]
[null,null,60,null,60,null,60,null,"215N/58 - Bügelhöhe 205"]
[null,null,65,null,65,null,65]
[null,null,70,null,70,null,70]
[]
[]
[]
[]
[]
[]
[]
[null,null,"innen",null,"innen",null,"innen"]
[null,null,30,null,30,null,10]
[null,null,35,null,35]
[null,null,40,null,40]
[null,null,45,null,45]
[null,null,50,null,50]
[null,null,55,null,55]
[null,null,60,null,60]
[null,null,65,null,65]
[null,null,70,null,70]
[]
[]
[]
[]
[null,null,"NGF",null,"NGF",null,"NGF"]
[null,null,"ohne Not- und Gefahrenfunktion",null,"nur für Doppelzylinder",null,"nur für Doppelzylinder"]
[null,null,"mit Not- und Gefahrenfunktion"]
[null,null,"mit Freilauffunktion"]
[]
[]
[]
[null,null,"Bohrschutz",null,"Bohrschutz",null,"Bohrschutz"]
[null,null,"Bohrschutz Klasse 3 (BS3)",null,"Bohrschutz Klasse 3 (BS3)",null,"Bohrschutz Klasse 3 (BS3)"]
[null,null,"Bohrschutz Klasse 4 (BS4)",null,"Bohrschutz Klasse 4 (BS4)",null,"Bohrschutz Klasse 4 (BS4)"]
[null,null,"Bohr- und Ziehschutz (BZ1)",null,"Bohr- und Ziehschutz (BZ1)",null,"Bohr- und Ziehschutz (BZ1)"]
[null,null,"Bohr- und Ziehschutz (BZ2)",null,"Bohr- und Ziehschutz (BZ2)",null,"Bohr- und Ziehschutz (BZ2)"]